**CS 428/528**

**Instructor: Anand Seetharam**

**Quiz 6**

**Baptiste Saliba**

1. The RTS/CTS mechanism in the CSMA/CA protocol helps mitigate the **collision** problem. **(1 point)**

2. What is the expansion of the acronym SNR? **(1 point)**

**Answer)** Signal-to-Noise Ratio

3. State two functions of the Mobile Switching Center in the cellular network architecture. **(2 points)**

**Answer)**

**1. connects cells to wired tel. net.  
2. manages call setup**

4. How many MAC addresses could potentially be there in an 802.11 frame? Briefly described what they are used for. **(2 points)  
  
Answer)**

**4 MAC Addresses**

**Address 1: Source MAC address  
Address 2: Destination MAC address  
Address 3: Router MAC address  
Address 4: Used for adhoc mode**

5. The 802.15 network uses the **master/slave** configuration to connect the devices **(1 point)**

6. State two important differences between wired and wireless links. **(2 points)**

**Answer)**

**1. Wireless networks are connected via Access Points at the final hop of the network; whereas wired networks are connected via ethernet cables at the last hop.  
2. Wireless networks allow for mobility whereas wired networks require a rigid network**

7. What is the expansion of the acronym CDMA? **(1 point)**

**Answer)**

Code-division multiple access